# Copyright:    Public domain.
# Filename:     ALARM_AND_ABORT.agc
# Purpose:      Part of the source code for Comanche, build 055. It
#               is part of the source code for the Command Module's
#               (CM) Apollo Guidance Computer (AGC), Apollo 11.
# Assembler:    yaYUL
# Reference:    pp. 1493-1496
# Contact:      Ron Burkey <info@sandroid.org>
# Website:      http://www.ibiblio.org/apollo.
# Mod history:  2009-05-07 RSB	Adapted from Colossus249 file of the same
#				name, and page images. Corrected various
#				typos in the transcription of program
#				comments, and these should be back-ported
#				to Colossus249.
#
# The contents of the "Comanche055" files, in general, are transcribed
# from scanned documents.
#
#       Assemble revision 055 of AGC program Comanche by NASA
#       2021113-051.  April 1, 1969.
#
#       This AGC program shall also be referred to as Colossus 2A
#
#       Prepared by
#                       Massachusetts Institute of Technology
#                       75 Cambridge Parkway
#                       Cambridge, Massachusetts
#
#       under NASA contract NAS 9-4065.
#
# Refer directly to the online document mentioned above for further
# information.  Please report any errors to info@sandroid.org.

# Page 1493
# 	THE FOLLOWING SUBROUTINE MAY BE CALLED TO DISPLAY A NON-ABORTIVE ALARM CONDITION. IT MAY BE CALLED
# EITHER IN INTERRUPT OR UNDER EXECUTIVE CONTROL.
#
# 	THE CALLING SEQUENCE IS AS FOLLOWS:
#		TC	ALARM
#		OCT	NNNNN
#					# (RETURNS HERE)

		BLOCK	02
		SETLOC	FFTAG7
		BANK

		EBANK=	FAILREG

		COUNT	02/ALARM

# ALARM TURNS ON THE PROGRAM ALARM LIGHT, BUT DOES NOT DISPLAY.

ALARM		INHINT

		CA	Q
ALARM2		TS	ALMCADR
		INDEX	Q
		CA	0
BORTENT		TS	L

PRIOENT		CA	BBANK
 +1		EXTEND
		ROR	SUPERBNK	# ADD SUPER BITS.
		TS	ALMCADR +1

LARMENT		CA	Q		# STORE RETURN FOR ALARM
		TS	ITEMP1

		CA	LOC
		TS	LOCALARM
		CA	BANKSET
		TS	BANKALRM

CHKFAIL1	CCS	FAILREG		# IS ANYTHING IN FAILREG
		TCF	CHKFAIL2	# YES TRY NEXT REG
		LXCH	FAILREG
		TCF	PROGLARM	# TURN ALARM LIGHT ON FOR FIRST ALARM

CHKFAIL2	CCS	FAILREG +1
		TCF	FAIL3
		LXCH	FAILREG +1
		TCF	MULTEXIT

FAIL3		CA	FAILREG +2
# Page 1494
		MASK	POSMAX
		CCS	A
		TCF	MULTFAIL
		LXCH	FAILREG +2
		TCF	MULTEXIT

PROGLARM	CS	DSPTAB +11D
		MASK	OCT40400
		ADS	DSPTAB +11D

MULTEXIT	XCH	ITEMP1		# OBTAIN RETURN ADDRESS IN A
		RELINT
		INDEX	A
		TC	1

MULTFAIL	CA	L
		AD	BIT15
		TS	FAILREG +2

		TCF	MULTEXIT

# PRIOLARM DISPLAYS V05N09 VIA PRIODSPR WITH 3 RETURNS TO THE USER FROM THE ASTRONAUT AT CALL LOC +1,+2,+3 AND
# AN IMMEDIATE RETURN TO THE USER AT CALL LOC +4. EXAMPLE FOLLOWS,
#		CAF	OCTXX		# ALARM CODE
#		TC	BANKCALL
#		CADR	PRIOLARM
#		...	...
#		...	...
#		...	...		# ASTRONAUT RETURN
#		TC	PHASCHNG	# IMMEDIATE RETURN TO USER. RESTART
#		OCT	X.1		# PHASE CHANGE FOR PRIO DISPLAY

		BANK	10
		SETLOC	DISPLAYS
		BANK

		COUNT	10/DSPLA

PRIOLARM	INHINT			# * * * KEEP IN DISPLAY ROUTINES BANK
		TS	L		# SAVE ALARM CODE

		CA	BUF2		# 2 CADR OF PRIOLARM USER
		TS	ALMCADR
		CA	BUF2 +1
		TC	PRIOENT +1	# * LEAVE L ALONE
-2SEC		DEC	-200		# *** DONT MOVE
		CAF	V05N09
		TCF	PRIODSPR

# Page 1495

		BLOCK	02
		SETLOC	FFTAG13
		BANK

		COUNT	02/ALARM

BAILOUT		INHINT
		CA	Q
		TS	ALMCADR

		TC	BANKCALL
		CADR	VAC5STOR

		INDEX	ALMCADR
		CAF	0
		TC	BORTENT
OCT40400	OCT	40400

		INHINT
WHIMPER		CA	TWO
		AD	Z
		TS	BRUPT
		RESUME
		TC	POSTJUMP	# RESUME SENDS CONTROL HERE
		CADR	ENEMA

		SETLOC	FFTAG7
		BANK

P00DOO		INHINT
		CA	Q
		TS	ALMCADR

		TC	BANKCALL
		CADR	VAC5STOR	# STORE ERASABLES FOR DEBUGGING PURPOSES.

		INDEX	ALMCADR
		CAF	0
ABORT2		TC	BORTENT

OCT77770	OCT	77770		# DONT MOVE
		CA	V37FLBIT	# IS AVERAGE G ON
		MASK	FLAGWRD7
		CCS	A
		TC	WHIMPER -1	# YES.  DONT DO POODOO.  DO BAILOUT.

		TC	DOWNFLAG
		ADRES	STATEFLG

		TC	DOWNFLAG

# Page 1496
		ADRES	REINTFLG

		TC	DOWNFLAG
		ADRES	NODOFLAG

		TC	BANKCALL
		CADR	MR.KLEAN
		TC	WHIMPER

CCSHOLE		INHINT
		CA	Q
		TS	ALMCADR
		TC	BANKCALL
		CADR	VAC5STOR
		CA	OCT1103
		TC	ABORT2
OCT1103		OCT	1103
CURTAINS	INHINT
		CA	Q
		TC	ALARM2
OCT217		OCT	00217
		TC	ALMCADR		# RETURN TO USER

DOALARM		EQUALS	ENDOFJOB
# CALLING SEQUENCE FOR VARALARM
#		CAF	(ALARM)
#		TC	VARALARM
#
# VARALARM TURNS ON PROGRAM ALARM LIGHT BUT DOES NOT DISPLAY
VARALARM	INHINT

		TS	L		# SAVE USERS ALARM CODE

		CA	Q		# SAVE USERS Q
		TS	ALMCADR

		TC	PRIOENT
OCT14		OCT	14		# DONT MOVE

		TC	ALMCADR		# RETURN TO USER

ABORT		EQUALS	BAILOUT		# *** TEMPORARY UNTIL ABORT CALLS OUT
